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Scope
This document describes the correct way to test and report issues with getting the M400, M600, M800 and M84 ECUs to synchronize.

Test Steps

· Connect laptop to the ECU and power the ECU

· Press F3 to get the Diagnostics View screen

· Press “Enter” key to clear all existing errors

· Start to crank the engine

· Press enter to clear all errors that were flagged as the engine started to crank, these errors are of NO IMPORTANCE

· While the engine is still cranking continue to press the “Enter” key and take note of the errors the keep returning.........it is important that the engine is continuously cranking
Only the errors that keep returning while the engine is cranking are important.  The errors that appear as the engine starts to crank or stops cranking are of no concern.

Make sure the EXACT name of the error is reported.

Data Logging
If the ECU has data logging available the following should be applied.

Logged Channels/rates:

· Engine RPM – 200Hz

· Error Group 6 – 5Hz
· Error Group 14 – 5Hz

· Status Group 1 – 50Hz

The same test procedure as described above should be carried out.   Clear the logging by downloading prior to the test.  Do at least two tests of 10 seconds (of cranking) one after the other.  Download logging.
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